1.6.7 -- Fixes (handling of usb timeouts and related, dualcam evk)
-------------------------------------------------------------------

  1. Merged mi48.py, interfaces.py and some part of utils.py from 
     development branch to fix some issues with USB interface,
     specifically for dualcam evk.

1.6.6 -- Feature (module_type support)
-------------------------------------------------------------------

  1. Merged mi48.py from development branch to enable cougar50x50
     and high sensitivity wafers.

1.6.5 -- Feature (DNN denoising and contrast enhancement)
-------------------------------------------------------------------

Feature:

  1. Denoising capability using proprietary DNN
  2. Contrast enhancement by means of fast histogram equalization

1.6.4 -- Bugfix (connections with named ports on linux)
-------------------------------------------------------------------

Fixed:

  1. Crash on linux when using named ports and multiple connected devices

1.6.3 -- Bugfix (connections to multiple sensors via USB on Linux)
-------------------------------------------------------------------

Fixed:

	2. Crash on Linux due to conflict (with connected device) when a second instance of pysenxor script or gui attempts to connect, when there is more than one device connected to the usb; now picks up and connect to the second device automatically.

1.6.2 -- Bugfix (connections to multiple sensors via USB)
----------------------------------------------------------

Fixed:

	1. Connection to named USB devices, e.g. by specifying -com COM9 or -com ttyACM0

	2. Crash due to conflict (with connected device) when a second instance of pysenxor script or gui attempts to connect, when there is more than one device connected to the usb; now picks up and connect to the second device automatically.

